**DATA SHEET**

**MODEL: NBT-230**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model** | **Part#** | **Rating**  **MBH** | **GPH** | **Material** | **Active Ingredient** | **Temp.**  **Rating** |
| NBT-230 | 2011 | 3500  Max | 26.0 | Polypropylene | Mg(OH)2  Pellets | 140F  Const. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Inlet port** | **Outlet port** | **Mounting** | **Clear Cover** | **Field Rechargeable** |
| .75” PVC Socket | 7.5” PVC Socket | Horizontal  Floor | Clear Cover | YES |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Fittings** | **Fittings** | **Wall Brackets** | Porous Refill Bag | Refill part # |
| .5” NPT x ¾” Barb (2) | .5” NPT PVC x ¾” Soc. | NO | Yes | 1114 |