**DATA SHEET**

**MODEL: NBT-610**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model** | **Part#** | **Rating**  **MBH** | **GPH** | **Material** | **Active Ingredient** | **Temp.**  **Rating** |
| NBT-610 | 2010 | 1500  Max | 11.0 | Polypropylene | Mg(OH)2  Pellets | 140F  Const. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Inlet port** | **Outlet port** | **Mounting** | **Clear Cover** | **Field Rechargeable** |
| 1” PVC Socket | 1” PVC Socket | Horizontal  Floor | Yes | YES |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Floor Mounted** | **Wall Mounted** | **Wall Brackets** | Porous Pellet Bag | Refill part # |
| Yes | No | NO | Yes | 1113 |