Model NBT-24-P

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Model | Part# | Rating | Flow GPH | Material | Active Ingredient | Temp. Rating |
| NBT-24-P | 2012 | 350 | 2.60 | Poly Tank | MgO Pellets | 140F  Const. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inlet port  Acid | Outlet Port | Mounting | Air  Conditioning  Condensate  Ports | Pellet Fill Lid |
| 1. ¾”lower Port 2. ¾” Top Port | 3/8” O.D.  Barb | Horizontal  Floor | 1. ¾”Top Open   Ports | Removeable  Cover |

Pump Data

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Model | Volts | Amps | Watts | High Water Switch |
| MD600  ETL Certified | 120/1/60 | 0.89 | 87 | 24 Volt Max.  Dry Contact |

Pump Performance GPH @ Feet Head

|  |  |  |  |
| --- | --- | --- | --- |
| 0’ | 6.5’ | 13.0’ | 20.0’ |
| 74.50 GPH | 66.0 GPH | 62.0 GPH | 32.5 GPH |